**Contract Bid Documents**

**Van Wert County**

**Township Cold Mix Program**

**Pleasant**

**Ridge**

**Van Wert County, Ohio**

**Township Cold Mix 2022**

**June – 2022**

**Legal Notice**

**2022 Township Cold Mix Program**

Sealed bids will be received by the **Pleasant and Ridge Township Trustees** in the office of

Ridge Township 16905 Middle Point Road, Van Wert, OH 45891

from 8:00 am to 4:00 pm Monday through Friday.

Bids to be opened Friday, July 8, 2022 at 9:00 a.m.

Bidder to furnish all labor, materials, and equipment for the following project:

**2022 Township Cold Constructed Asphalt Pavement Program**

Contract documents, bid sheets, plans and specifications may be obtained at the Ridge Township Office at 16905 Middle Point Road between 8:00 am and 4:00 pm or on websites ridgetownshipquarry.com or .pleasanttownshipvw.com

All bidders must be pre-qualified in conformance with Ohio Department of Transportation Requirements.

Each bidder is required to furnish with its proposal a Bid Guarantee and Contract Bond in accordance with Section 153.571 of the Ohio Revised Code. Bid security furnished in Bond form, shall be issued by

a Surety Company or Corporation licensed in the State of Ohio to provide said surety.

Each proposal must contain the full name of the party or parties submitting the proposal.

All Contractors and Subcontractors involved with the project will, to the extent practicable, use Ohio.

Products, materials, services, and labor in the implementation of their project. Compliance with the Equal Employment Opportunity requirements of Ohio Administrative Code Chapter 123, the Governor’s Executive Order of 1972, and Governor’s Executive Order 84-9 shall be required.

Bidders must comply with the prevailing wage rates on public improvements in Van Wert County, Ohio as determined by the Ohio department of Commerce.

Bids are to be sealed, marked **“Bid – Township Cold Constructed Asphalt Pavement 2022”** and addressed to Pleasant and Ridge Township Trustees**.**

Trustees for Pleasant and Ridge Township reserve the right to waive irregularities and to reject any or all bids submitted on any basis without discloser of a reason. The failure to make such a discloser shall not result in the accrual of any right, claim, or cause of action by any successful bidder against Pleasant or Ridge Township Trustees.

 Pleasant and Ridge Township Trustees

To Be Advertised: June 22, 2022

We, the undersigned, do hereby acknowledge that the wage scale and specifications were attached to this bidding blank and are a part of this submitted Bid Proposal.

 Signed: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Name & Title: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Contractor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Phone No. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Email: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Tax ID #: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 AFFIDAVIT

Contract

 State of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_)

County of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_)

 Before me, a Notary, in and for said county, personally appeared \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_,

Contractor(s) who being duly sworn deposes and says that they are following section 5719.042 of the Ohio Revised Code, which as follows:

 “ After the award by a taxing district of any contract let by competitive bid and prior to the time the contract is entered into, the person making a bid shall submit to the districts fiscal officer a statement affirmed under oath that the person with whom the contract is to be made was not charged at the time the bid was submitted with any delinquent property taxes on the general tax list of personal property of any county in which the taxing district has territory or that such person was charged with delinquent personal property taxes on any such tax list, in which case the statement shall also set forth the amount of such due and unpaid delinquent taxes on any such tax list and any due and unpaid penalties and interest thereon. If the statement indicates that the taxpayer was charged with any such taxes, a copy of the statement shall be transmitted by the fiscal officer of the County Treasurer within 30 days of the date it is submitted.”

If any statements are required from the above, please attach same to this affidavit.

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Contractor

 By: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Sworn to me and signed in my presence this \_\_\_\_\_\_\_\_\_\_day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_, 20\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Notary Public

 My Commission Expires: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Affidavit in Compliance with Section 3517.13 Of the Ohio Revised Code

State of Ohio

County of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_SS:

 Personally, appeared before me the undersigned, as an individual or as a representative of

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ for a contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

To be let by the Pleasant and Ridge Township Trustees, who, being duly cautioned and sworn, make the following statement with respect to prohibited activities consulting a conflict of interest or other violations under Ohio Revised Code, Section 3517.13, and further states that the undersigned has the authority to make the following representation on behalf of himself or herself or of the business entity:

1. That none of the following has individually made within the two previous calendar years that, if awarded a contract for the purchase of goods or services in excess of 500.00, none of the following individually will make, beginning on the date the contract is awarded and extending until one year following the conclusion of the contract, as an individual, one or more campaign contributions totaling in excess of 1000.00, to any member of the Pleasant or Ridge Township trustees or their individual campaign committees:
2. Me:
3. Any partner or owner or shareholder of the partnership (if applicable)
4. Any owner of more than 20% of the corporation or business trust (if applicable)
5. Each spouse of any person identified I (a) through (c) of this section.
6. Each child seven years of age to seventeen years of age of any person identified in division (a) through (c) of this section (only applicable to contributions made on or after January 1, 2007)
7. That none of the following have collectively made since January 1, 2007, and that, if awarded a contract for the purchase of goods and services more than 500.00, none of the following collectively will make, beginning on the date of the contract, one or more campaign contributions totaling more than 2000.00 to any member of the Pleasant or Ridge Township Trustees or their individual campaign committees:
8. Me
9. Any partner or owner or shareholder of the partnership (if applicable)
10. Any owner of more than 20% of the corporation or business trust (if applicable)
11. Each spouse of any person identified I (a) through (c) of this section.
12. Each child seven years of age to seventeen years of age of any person identified in division (a) through (c) of this section (only applicable to contributions made on or after January 1, 2007)

 Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Title: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Sworn and before me and subscribed in my presence this\_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_ 20\_\_\_\_\_

 Notary Public: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 My Commission Expires: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Non – Collusion Affidavit

State of OHIO,

 ) SS.

Van Wert County)

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, being first duly sworn, deposes and says that.

He is \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The party making the foregoing proposal or bid; that such bid is genuine and not collusive or sham; that said bidder is not financially interested in, or otherwise affiliated in a business way with any other bidder on the same contract; that said bidder has not colluded, conspired, connived, or agreed, directly or indirectly, with any bidder or person, to put in a sham bid, or that such other person shall refrain from bidding, has not in any manner, directly or indirectly sought by agreement or collusion, or communication or conference, with any person, to fix any overhead, profit or cost element of said price, or of that of any other bidder, to secure any advantage against a Township of Van Wert County or any person or persons interested in the proposed contract; and that all statements contained in said proposal or bid are true; and further, that such bidder has not, directly or indirectly submitted this bid, or the contents thereof, or divulged information or data relative to any association or to any member or agent thereof.

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Affiant

Sworn to before me and signed in my presence this \_\_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, 20\_\_\_\_.

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Notary Public

 My Commission Expires: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Supplemental Specifications

The Contractor shall notify each Township three (3) days prior to the commencement of work in that Township. The Contractor shall provide a detailed work schedule to each Township a minimum of three (3) days prior to commencement of work.

When chip sealing all routes, the Contractor may close the portions of the routes under construction to through traffic to seal the road full width or the Contractor may elect to maintain traffic by providing flaggers. Should the Contractor choose to close the road, the following requirements must be met:

The Contractor shall notify the Township of the closure a minimum of three (3) working days prior to closing the road. This will allow the Township time to provide notice to the public.

The Contractor shall only close the road being chip sealed between two adjacent intersections. The Contractor shall always allow residents along the closed portion access to their homes or businesses.

The Contractor shall always provide access for emergency vehicles.

The Contractor shall provide appropriate signs, cones, and other devices to warn and inform the public. Such devices shall be approved by the Township.

The Contractor shall not be permitted to have the road remained closed over night or during hours of darkness.

The Contractor shall provide flaggers and signs to direct traffic and to direct trucks turning into or backing into the construction area.

Each Township will be billed separately for materials and labor applied within their Township. Township billing addresses will be supplied to the contractor. A weigh ticket shall accompany each delivery of bituminous material from the bituminous material supplier. Copies of all material quantity ticket for the work in each Township shall be delivered to the respective Township at the end of each day unless other arrangements are made with the individual Township.

The Completion Date has been set in the contract and the Contractor shall adhere to this date or Liquidated Damages will be assessed according to ODOT Construction and Materials Specifications Item 108.07 Failure to Complete on Time. Damages will be deducted from the work remaining in each Township where the work has not been completed by the date set within this contract.

It is assumed the intent of all bid items is clear from the item description and specification. Any questions regarding any portion of these Contract Documents should be addressed Not Less than five (5) days prior to submission of bid.

**SPECIFICATION**

**For**

**ITEM SPECIAL FOG SEAL QF-40**

**Test Parameter on Emulsion Test Method Specification**

Oil Distillate, Volume % max AASHTO T 59 0.5

Residue by Distillation, % min. AASHTO T 59 35 – 45

Sieve, % max. AASTHO T 59 0.3

Viscosity, Saybolt Furol, 25⁰C, sec AASTHO T 72 10 – 100

**Test on Emulsion Residue**

Penetration, 25⁰C, 100g, 5 sec, dmm min AASTHO T 49 55

Solubility in TCE, % min AASTHO T 44 97.5

Fog seal shall be provided as a unit price per square yard at an application rate of 0.12 gallons per square yard.

The Contractor may be asked to provide testing verification to be submitted for the proposed fog seal material.

A weigh ticket shall accompany each delivery of fog seal material from the bituminous material supplier. Copies of all material quantity ticket for the work shall be delivered to the township at the end of each day unless other arrangements are made with Township.

Payment for this will be the unit price bid for Special QF-40 Fog Seal application rate 0.12 gallons/square yard.

 **ITEM 405 – COLD CONSTRUCTED ASPHALT PAVEMENT**

**Description**

**Job Mix Formula**

**Composition**

**Material**

**Mixing Plant**

**Weather Limitation**

**Test Strip and Start up Procedures**

**Hauling**

**Bituminous Paver**

**Rollers**

**Conditioning Existing Surface**

**Spreading and Finishing**

**Joints**

**Spreading and Surface Tolerances**

**Method of Measurement**

**Basis of Payment**

**Description.** This work shall consist of providing all labor, equipment, materials, transportation, temporary off site work area property for production and storage for the furnishing and paving a Cold Constructed Asphalt Pavement (CCAP) according to the requirements set forth within these specifications and plans.

**Job Mix Formula.** A job mix formula (JMF) shall be submitted by the Contractor using representative samples of the aggregates to be used in the CCAP mixture. The mix design that is submitted by the Contractor shall be performed by a laboratory that possesses a current and valid AASHTO R18 accreditation in both aggregates and HMA, at a minimum.

**Composition.** Use Nos. 57, 67, 8 or 9 size aggregate for the mixture as specified. Use No. 9 aggregate or screenings for the choke aggregate as specified. The aggregates to be used shall be based on the proposed overlay thickness. Minimum thickness shall be 2 times the largest aggregate in the design.

The choke aggregate shall be of a gradation that will fill surface voids without excess, the Engineer may adjust the estimated quantity of the choke aggregate.

The use of any recycled materials, recycled aggregates, crushed concrete, slag aggregates or reclaimed asphalt pavement will not be allowed for use in the JMF or choke aggregate.

**Materials.** Bituminous material to be used shall meet the specifications shown in Table 1.

|  |
| --- |
| **Table 2: Specifications for Multigrade Cold Mix Asphalt** |
| Method of Test | CM-150 |
| Modified Kopper Vacuum Viscosity, 25⁰C, ASTM D 4957 | 800 – 10,000 P |
| Flash Point. Tag Flash Point, ASTM D 3143-98 | 65.5⁰C (min) |
| Water in Petroleum, ASTM D 95-05 | 1.0% (max) |
| Cut-Back Distillation, ASTM D 402-02 Distillate, % by Volume of Total Distillate to 360⁰: to 225⁰C to 260⁰C to 315.5⁰C Residue from Distillation to 360⁰C | 0 – 3% by Vol0 – 3% by Vol40 – 80% by Vol85% (min) |
| Test on Residue from Distillation, ASTM D 402 |  |
|  Penetration, 25⁰C, 100 g, 5 sec. ASTM D 5-05a | 150 – 250 dmm |
|  Solubility in Trichloroethylene, ASTM D 2042-01 | 99.0% (min) |
|  Softening Point, ASTM D 36-95 | 73.8⁰C (min) |
|  Float Test, 60⁰C, ASTM D 139-95 | 1200 sec (min) |

The asphalt binder shall be delivered to point of production at a minimum temperature of 250⁰F.

Typical application rate of bituminous material shall be approximately 5% by weight +/- 5%, depending on the aggregate gradation, moisture content and temperature. The final percent by weight shall be determined by the Project Engineer or owners Representative at the time of production.

**Mixing Plant.** The mixing unit shall have as a minimum two (2) 6-cubic yard capacity hoppers with oversize screening and vibrators on the hopper walls to assist in the free flow of material. The proportioning of materials shall be controlled by means of mechanically adjustable gate valves at the point of discharge to a variable speed belt conveyor, equipped with a belt scale for continuous weighting of the aggregate. The aggregate belt scale shall be coupled/interlocked with two microprocessor controlled systems, complete with two independent pumping systems and spray bars, to regulate the application of bituminous material.

The mixing unit shall be an on-board completely self-contained counter rotating twin shaft pugmill. A metering device shall be capable of automatically adjusting the flow of bituminous material to compensate for any variation in the weight of the aggregate introduced into the pugmill. Bituminous material shall be metered by weight of aggregate using a mass flow, Coriolis Effect, type meter that will accurately measure the amount to within 0.5 percent of the amount required by the JMF or as adjusted by the Engineer.

Control of the plant shall be fully automatic via the microprocessors. Control functions shall include: batch production, automatic plant startup, monitoring of individual drive systems, warning signals in case of material shortage, monitoring of filling leveling, temperatures and pressures, pre-selection of tonnage, automatic plant shut down. A current setting of the mixing unit shall be continuously displayed.

The Contractor shall be required to assure complete coating of the blended aggregate with the Multigrade Cold Mix Asphalt Binder and any remixing through the pugmill or by manipulation of stockpiled material shall be considered acceptable. The Contractor will not be compensated separately for this work; it shall be included in the item Cold Constructed Asphalt Pavement.

**Weather Limitation.** Do not place Cold Constructed Asphalt Pavement under the following conditions: when the existing surface has standing water or is saturated, when the air temperature is below 60⁰F or when weather conditions otherwise prevents proper handling, finishing of the CCAP mixture.

Exception to the above weather limitation is if the CCAP is being placed on grade directly from the pugmill unit and not placed in a stockpile. In this situation the Contractor may place the CCAP if the air temperature is at 45⁰F. The same conditions apply as to the handling, spreading and finishing of CCAP material as stated in these specifications.

**Test Strip and Start Up Procedures.** During the first day of laydown operations the Contractor shall construct a test strip a single lane wide, 1000 feet in length, on the project. The Contractor shall use this to demonstrate that the material, workmanship, equipment and processes proposed will produce a stable CCAP layer that conforms to the requirements of the project specifications without rutting or deformation under traffic.

Should the test strip be accepted by the Engineer the Contractor may continue with the paving that day. Should the test strip fail the Contractor and the Engineer shall determine the best plan to correct the deficiencies in the test strip and correct the paving operation moving forward. The Contractor will be required to perform another test strip with the recommended corrections and have that approved by the Engineer before continuing with paving operation.

Any and all cost incurred by the Contractor for a failed test strip, this includes any corrective actions up to and including complete removal and replacement shall be the sole responsibility of the Contractor and no additional compensation will be given by the Owner Agency.

**Hauling.** Hauling of the CCAP mixture shall be done using trucks that conform to ODOT Construction and Materials specification 401.11.

**Bituminous Paver.** The CCAP material shall be spread using a self-propelled paver having electronic grade and cross slope controls for the screed. The equipment shall be of sufficient size and power (170 hp) to spread the CCAP material in one continuous pass, without segregation, to the lines and grades established by the Contractor and according to the Plans.

Handwork of CCAP Material shall be minimized and care shall be taken to prevent segregation. The wings of the paver shall be emptied regularly to prevent buildup and to minimize segregation.

**Rollers.** The CCAP material shall be compacted using a minimum 10-ton static dual drum steel roller. The material shall be initially rolled in 2 passes, up and back, to seat the mat. The mat will then be rolled with an additional pass after the surface choke stone has been applied.

**Conditioning of the Existing Surface.** Clean the surface on which the CCAP material is to be placed, and keep it free of accumulations of materials that would, in the judgment of the Engineer, contaminate the mixture, prevent bonding, or interfere with spreading operations. Where approved subgrade or pavement courses previously constructed under the Contract become loosened, rutted, or otherwise defective, correct the deficiency according to the contract item or items involved before the spreading of a subsequent pavement course.

**Spreading, Finishing and Surface Tolerances.** Spread and finish the CCAP material to the lines and grades shown on the plans.

Immediately following the initial rolling, apply the choke aggregate uniformly with an adjustable, hopper equipped, revolving drum type spreader at the specified rate or as directed by the Engineer.

Should the placed mat show signs of rutting or deformation, the Contractor shall be required to re-roll and/or rework the surface and repair any surface issues caused by traffic as well as the Contractors operations. This includes shoulder placement and driveway approach construction. The Contractor shall be responsible for maintaining the condition of the pavement until final acceptance has been given by the Owner Agency.

The placed CCAP material shall meet the surface tolerances specified in 401.19. The variation of the surface from the testing edge of the 10 foot straightedge shall not exceed 3/8 inch.

**Joints.** Where the CCAP material is to match into an existing HMA or Concrete driveway, cross road or other surface, a butt joint shall be milled to provide a smooth transition from the new CCAP pavement to the existing pavement. Feathering of the CCAP material will not be permitted.

**Method of Measurement.** The CCAP material will be measured by the total weight of aggregate plus the weight of the bituminous binder used to blend to create the final CCAP mixture. This weight will be measured in total tons. This tonnage will include all labor, equipment, materials, mobilization, testing and any other incidental cost to produce the CCAP mixture.

Choke aggregate will be measured by the total tons placed on the roadway.

**Basis of Payment.** The Owner Agency will pay for accepted quantities of Cold Constructed Asphalt Pavement complete and in place at the contract prices as follows:

**Item Unit Description**

405 Ton Cold Constructed Asphalt Pavement

405 Ton Choke Aggregate

**Item Special – Deduct for #8 Aggregate Delivered by Others**

This item is a contract price deduction for the delivery of #8 aggregate to the Cold Constructed Asphalt mixing location by the Ridge Township Stone Quarry. This deduct is only for the transportation of the aggregate from the quarry to the mixing yard location. The Contractor shall still be responsible for the purchase of aggregate from the Ridge Township Stone Quarry. The Ridge Township Quarry will transport and stockpile the #8 aggregate at the mixing yard location.

This item will be a per ton price deduction from the base bid for item 405 Cold Constructed Asphalt Pavement #8 Surface Course ay 2” Depth. Award of the contract will be based on the total base bid for both Ridge and Pleasant Townships NOT including the deduction for #8 aggregate delivered by others.

**203 – Excavation for Pavement Widening**

This work shall consist of excavating and disposal of material to complete the widening of the existing roadway as per attached widening detail. The excavated areas shall be completely backfilled at the end of workday. No excavation shall remain open overnight.



Township Trustee Agreement Page

Will need a minimum of 2 signatures from each township before construction begins in each specific township

**Pleasant Township: Contact- Todd Wallace 419-203-6539**

 1.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 2.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 3.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 **Ridge Township: Contact Bill Evans 419-771-4080**

 1.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 2.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 3.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_